# Simple eCos string signatures
0        string    ecos                    eCos RTOS string reference:
>0       string    x                       "%s"
0        string    eCos                    eCos RTOS string reference:
>0       string    x                       "%s"
0        string    ECOS                    eCos RTOS string reference:
>0       string    x                       "%s"

# eCos kernel exception handlers
#
# mfc0    $k0, Cause       # Cause of last exception
# nop                      # Some versions of eCos omit the nop
# andi    $k0, 0x7F
# li      $k1, 0xXXXXXXXX
# add     $k1, $k0
# lw      $k1, 0($k1)
# jr      $k1
# nop
0       string      \x00\x68\x1A\x40\x00\x00\x00\x00\x7F\x00\x5A\x33    eCos kernel exception handler, architecture: MIPSEL,
>14     leshort     !0x3C1B                                             {invalid}
>18     leshort     !0x277B                                             {invalid}
>12     uleshort    x                                                   exception vector table base address: 0x%.4X
>16     uleshort    x                                                   \b%.4X

0       string      \x00\x68\x1A\x40\x7F\x00\x5A\x33                    eCos kernel exception handler, architecture: MIPSEL,
>10     leshort     !0x3C1B                                             {invalid}
>14     leshort     !0x277B                                             {invalid}
>8      uleshort    x                                                   exception vector table base address: 0x%.4X
>12     uleshort    x                                                   \b%.4X

0       string      \x40\x1A\x68\x00\x00\x00\x00\x00\x33\x5A\x00\x7F    eCos kernel exception handler, architecture: MIPS,
>12     beshort     !0x3C1B                                             {invalid}
>16     beshort     !0x277B                                             {invalid}
>14     ubeshort    x                                                   exception vector table base address: 0x%.4X
>18     ubeshort    x                                                   \b%.4X

0       string      \x40\x1A\x68\x00\x33\x5A\x00\x7F                    eCos kernel exception handler, architecture: MIPS,
>8      beshort     !0x3C1B                                             {invalid}
>12     beshort     !0x277B                                             {invalid}
>10     ubeshort    x                                                   exception vector table base address: 0x%.4X
>14     ubeshort    x                                                   \b%.4X
